{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Accueil","Façade à ossature bois","Propriétés POBIM","Pays d'usage","Grandeurs","Modèle d'objet"],"not_rendered":{"charts":0,"images":246,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Accueil","index":0,"n_rows":2,"n_cols":5,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,null,null,"Cliquer sur le bouton pour créer un nouveau modèle d'objet générique"]

{"sheet":"Façade à ossature bois","index":1,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["Identifiant unique","Documents de référence","Date de création","Nom dans la langue du créateur","Définition dans la langue du créateur","Nom en anglais international","Définition en anglais international","Représentation visuelle","Pays d'usage","Date de validation"]
["{245A5705-AC40-4B48-B38F-26AD6AFA7DF5}","\rRP RAGE Façades ossature bois non porteuses\n","2018-01-23T14:57:04","Façade à ossature bois","Façades à ossature bois non structurales constituées de montants et de traverses en bois, et de panneaux à base de bois, intégrant éventuelement leur remplissage (isolation, menuiserie), et les films associés.","to be defined","to be defined",null,"FR","2018-03-29"]
[]
["Propriétés associées"]
["Id","Nom dans la langue du créateur"]
["{ABE90E1B-C133-431B-BC95-23E927D2AD19}","Essence de bois des éléments d'ossatures"]
["{0D9490D0-8589-421A-8FFE-00EF7F8A4A62}","Essence de bois des éléments d'ossatures secondaires extérieures"]
["{1DF0D867-A091-477A-8EF9-EC97D19F4616}","Essence de bois des éléments ossatures secondaires intérieures"]
["{BE312A55-8B4D-4442-9892-93974CFA6667}","Compatibilité classe d'emploi des éléments en bois"]
["{82B28790-06B5-490E-A185-C43A6801F99D}","Compatibilité classe d'emploi de la lisse basse"]
["{0C171828-9377-421E-967A-68079FC445C1}","Resistance aux insectes des éléments en bois"]
["{636D108E-11D3-4795-A9DB-52F155E524B9}","Largeurs des éléments d'ossatures"]
["{E460AEAE-F5A3-40B0-813B-B277A1A04754}","Largeurs des éléments d'ossatures secondaires extérieures"]
["{9DD1EE55-ED88-45F4-A0F9-8189508BEBD3}","Largeurs des éléments d'ossatures secondaires intérieures"]
["{2A48B8A3-D7B5-40A7-AE92-138D06DC7C84}","Entraxe des éléments d'ossatures"]
["{42F60E09-9598-45BD-9CE5-237608AD5294}","Entraxe des éléments d'ossatures secondaires extérieures"]
["{C7CF1097-00EA-4638-A076-1AF97AAD22B1}","Entraxe des éléments d'ossatures secondaires intérieures"]
["{59E181D9-55A0-49DA-A55C-756A05953F84}","Orientation des éléments d'ossatures"]
["{CF62A7B4-8977-48EC-BE94-5A81274F1A1C}","Orientation des éléments d'ossatures secondaires extérieures"]
["{CF8BCCE1-13C5-4A8B-8EAC-50268526F147}","Orientation des éléments d'ossatures secondaires intérieures"]
["{D6EB3364-4965-4531-8E27-BC4E7E78A736}","Nature du voile de stabilité"]
["{D1E6921D-0303-4A18-931A-021C77FA59DC}","Epaisseur du voile de stabilité"]
["{E48B2D26-0319-4A06-B2CA-B1AB165AF9D7}","Valeur Sd du pare-pluie"]
["{873DA443-402B-4C03-87BE-C53EDA48C7D5}","Résistance aux UV du pare-pluie"]
["{E550E3E6-4E66-4DBE-A019-6E6784FB8B8F}","Nature de l'isolant entre éléments d'ossatures"]
["{20E96CDC-3192-49A9-93DD-2FE35F27B526}","Nature de l'isolant du doublage extérieur"]
["{177BB781-3293-45FB-8270-7F849D9D1FCE}","Nature de l'isolant du doublage intérieur"]
["{14631FD0-0F15-42DD-86A3-8793C88B9827}","Epaisseur de l'isolant entre éléments d'ossatures"]
["{6D231B77-A082-436A-A7DA-AB5C2C3E1C6B}","Epaisseur de l'isolant du doublage extérieur"]
["{F4357B5F-16E5-45E8-8074-A35CA8405D51}","Epaisseur de l'isolant du doublage intérieur"]
["{4E5DF3DE-067F-41E1-9912-0EA0A7CC325D}","Conductivité thermique de l'isolant entre éléments d'ossatures"]
["{1392B810-1E1F-40D2-B11E-97A0D4AF5D6A}","Conductivité thermique du doublage intérieur"]
["{611F3267-70EF-410B-8DCC-1E0877C9638B}","Conductivité thermique de l'isolant du doublage extérieur"]
["{1FEC2725-D69B-4ECD-9A4D-91E02F36B6D0}","Valeur Sd du pare-vapeur souple"]
["{E6BE67B6-FF52-422D-983A-AE3259E966F0}","Type de barrière à la diffusion de vapeur d'eau"]
["{8409555A-87F1-4E22-A1A4-CB242BD3DC81}","Résistance thermique de la FOB"]

{"sheet":"Propriétés POBIM","index":2,"n_rows":72,"n_cols":22,"rows_kept":72,"cut":false,"hidden":false,"merged":[]}
["Identifiant unique","Documents de référence","Date de création","Symbole","Nom dans la langue du créateur","Définition dans la langue du créateur","Nom en anglais international","Définition en anglais international","Type","Cardinalité","Grandeur","Enumération des valeurs possibles dans la langue du créateur","Expression de la grandeur","Représentation visuelle","Pays d'usage","Valeurs bornes","Format","Relations entre propriétés","Date de validation",null,"Demandé par","GTTR"]
["{F5FEE0E7-66DA-4E16-B262-7D09C5967E0B}","NF DTU 33.1\r\nNF EN 12153\r\nNF EN 12152\n","2018-01-17T10:19:46","A*","Permabilité à l'air","Résistance de la menuiserie à l'air. Noté A* suivi d'un chiffre de 1(faible) à 4(très bon). Valeur obtenue par essai.","Air permeability","To be defined","enumerated-type",1,"sans grandeur","A*1\r\nA*2\r\nA*3\r\nA*4\r\n",null,null,"FR",null,null,null,"2018-10-10",null,"Façades métalliques"]
["{541EDC81-B4A6-42DC-A57F-8F656319A2D3}","NF DTU 33.1\r\nNF EN 12155\nNF EN 12154\r\n","2018-01-17T10:43:17","E*","Etanchéité à l'eau","Etanchéité de la menuiserie à l'eau. Noté E* suivi d'un chiffre de 1 (très faible) à 9 (très bon). Valeur obtenue par essai.","Water tightness","To be defined","enumerated-type",1,"sans grandeur","E*1\r\nE*2\r\nE*3\r\nE*4\r\nE*5\r\nE*6\r\nE*7\r\nE*8\r\nE*9\r\n",null,null,"FR",null,null,null,"2018-10-10",null,"Façades métalliques"]
["{E12DA40C-313E-45B4-9466-DB11D29BCF67}","NF DTU 33.1\r\nNF EN 12179\r\n","2018-01-17T11:04:55","V*","Déformation au vent","Résistance de la menuiserie au vent. Noté V* suivi de deux critères, la déformation de la menuiserie (en lettre) et la résistance à la pression (en chiffre).","Wind deflection","To be defined","enumerated-type",1,"sans grandeur","V*A1\nV*A2\r\nV*A3\r\nV*A4\r\nV*A5\r\nV*A6\r\nV*A7\r\nV*A8\r\nV*A9\r\nV*B1\r\nV*B2\r\nV*B3\r\nV*B4\r\nV*B5\nV*B6\nV*B7\nV*B8\nV*B9\nV*C1\nV*C2\nV*C3\nV*C4\nV*C5\nV*C6\nV*C7\nV*C8\nV*C9\n",null,null,"FR",null,null,null,"2018-10-10",null,"Façades métalliques"]
["{72F8B28F-DE0C-42DF-90FB-02E266A49FF7}","NF DTU 33.1\r\n","2018-02-06T16:10:01",null,"Présence d'un ouvrant","Présence d'un ouvrant","Window","To be defined","boolean-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Façades métalliques"]
["{A23392DE-6736-4F07-9BA9-D83B411E79DE}","NF DTU 33.1\r\n","2018-02-06T14:42:44",null,"Remplissage verrier","Les produits verriers utilisés doivent être conformes à la norme NF DTU 39 P1-2 (CGM)\nLes produits utilisés doivent être en mesure d'assurer dans le temps les fonctions pour lesquelles ils sont prévus.","Glass filling","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Façades métalliques"]
["{630C20E8-F6AF-43C6-B961-C73E5594292C}","NF DTU 33.1\r\n","2018-02-06T15:38:53",null,"Remplissage opaque ventilé","Remplissage opaque ventilé","Opaque ventilated filling","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Façades métalliques"]
["{67F99082-FC4E-40FB-867E-F254C2DD9E65}","NF DTU 26.1\r\n","2018-01-26T10:39:52",null,"Epaisseur Gobetis","Epaisseur minimale de la première couche de l'enduit nécessaire pour préparer l'accrochage de l'enduit. Le gobetis est en fonction de l'état de surface du support.","Thickness of gobetis","Minimum thickness of the first layer of the coating necessary to prepare the bonding of the coating. The gobetis is depending on the surface condition of the support.","real-type",1,"longueur",null,"mm",null,"FR","0 à 5mm",null,null,"2018-10-10",null,"Enduits"]
["{2327AC35-528F-4DCD-9B88-86BD9D60F475}","NF DTU 26.1\r\n","2018-01-26T11:02:27",null,"Epaisseur Corps d'enduit","Epaisseur minimale de la seconde couche de d'enduit nécessaire pour assurer la planéité de l'enduit , le rattrapage des irrégularité du support et éventuellement son impermablisation.","Thickness of the plaster body.","Minimum thickness of the second layer of plaster necessary to ensure the flatness of the plaster, the catching of the irregularity of the support and possibly its impermablisation.","real-type",1,"longueur",null,"mm",null,"FR","10 à 15 mm",null,null,"2018-10-10",null,"Enduits"]
["{A8ABE0A0-8AD1-4A80-B784-4550C0F53142}","NF DTU 26.1\r\n","2018-01-26T11:02:47",null,"Epaisseur de la finition","Epaisseur minimale de  la troisième couche du système d'enduit. Elle a ou non un rôle décoratif. Elle assure la protection du coprs d'enduit.","Thickness of the topcoat","Minimum thickness of the third layer of the plaster system. It has or not a decorative role. It ensures the protection of the coating body.","real-type",1,"longueur",null,"mm",null,"FR","5 à 8 mm",null,null,"2018-10-10",null,"Enduits"]
["{D4D880D0-F17C-47BE-A79B-29476DA4B605}","NF DTU 26.1","2018-01-26T11:03:05",null,"Dosage en liant du gobetis","Teneur en liant hydraulique (ciment, ciment Naturel Prompt, ciment à maçonner, chaux de construction, etc.) par kg/m3 de sable sec nécessaire pour la réalisation du gobetis. Les différents dosages sont donnés dans le NF DTU 26.1 NF EN 998-1.","Dosage by binding gobetis","Hydraulic binder content (cement, natural Prompt cement, masonry cement, building lime, etc.) per kg / m3 of dry sand necessary for making the gobetis. The different dosages are given in NF DTU 26.1.","real-type",1,"masse volumique",null,"kg/m3",null,"FR",null,null,"{643FFD46-69C2-4135-B9BA-1A247C53731F}","2018-10-10",null,"Enduits"]
["{AEEDC353-A32E-4671-B693-168ED5D2BCEE}","NF DTU 26.1","2018-01-26T11:03:39",null,"Dosage en liant du corps d'enduit","Teneur en liant hydraulique (ciment, ciment Naturel Prompt, ciment à maçonner, chaux de construction, etc.) par kg/m3 de sable sec nécessaire pour la réalisation du gobetis. Les différents dosages sont donnés dans le NF DTU 26.1 NF EN 998-1.","Dosage by binder of plaster body","Hydraulic binder content (cement, natural Prompt cement, masonry cement, building lime, etc.) per kg / m3 of dry sand necessary for making the gobetis. The different dosages are given in NF DTU 26.1.","real-type",1,"masse volumique",null,"kg/m3",null,"FR",null,null,"{643FFD46-69C2-4135-B9BA-1A247C53731F}","2018-10-10",null,"Enduits"]
["{5FE2CECA-6D84-4A1D-ABE1-8D635867DE24}","NF DTU 26.1","2018-01-26T11:03:55",null,"Dosage en liant de la couche de finition","Teneur en liant hydraulique (ciment, ciment Naturel Prompt, ciment à maçonner, chaux de construction, etc.) par kg/m3 de sable sec nécessaire pour la réalisation du gobetis. Les différents dosages sont donnés dans le NF DTU 26.1 NF EN 998-1.","Dosage by binder of the topcoat","Hydraulic binder content (cement, natural Prompt cement, masonry cement, building lime, etc.) per kg / m3 of dry sand necessary for making the gobetis. The different dosages are given in NF DTU 26.1.","real-type",1,"masse volumique",null,"kg/m3",null,"FR",null,null,"{643FFD46-69C2-4135-B9BA-1A247C53731F}","2018-10-10",null,"Enduits"]
["{0BF528D6-0521-49BB-8FBD-0203F37599C5}","NF DTU 26.1","2018-01-26T11:05:26",null,"Type de Finition","Défini l'aspect de surface donné à l'enduit","To be defined","To be defined","enumerated-type",1,"sans grandeur","Projeté\nGratté\nGratté grésé\nGrésé\nLavé\nBrossé\nTaloché\nlissé\nTyrolien\nGranulats projetés",null,null,"FR",null,null,null,"2018-10-10",null,"Enduits"]
["{E253C139-0ED1-4A72-A2A2-39DCC681F88E}","NF DTU 26.1","2018-01-26T11:14:29",null,"Planéité","Mesure par la flèche prise sous la règle de 2m qui doit être au plus égale aux valeurs énumérées","To be defined","To be defined","enumerated-type",1,"longueur","Enduit courant: 10 mm\nEnduit Enduit soigné : 5 mm",null,null,"FR",null,null,null,"2018-10-10",null,"Enduits"]
["{BB5FE0C9-6720-4C55-B992-0918E3B17226}","RP Rage bardage en acier protégé et acier inoxydable\nCahier CSTB 3747\nFDP 20-651","2018-02-07T11:01:53",null,"Matériaux extérieur (si bois: essence)","Matériaux extérieur (si bois: essence)","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"bardage métallique"]
["{7480D82F-C642-4485-858D-7132FBAF2BE9}","NF T34722","2018-02-07T11:04:29",null,"Classement peinture","Classement peinture","To be defined","To be defined","enumerated-type",1,"sans grandeur","I1à4\r\nD1à4\r\n",null,null,"FR",null,null,null,"2018-10-10",null,"Peinture"]
["{B1AB0BEF-97B3-49E6-99AB-A30C1F61CFBC}","GTTE Façades","2018-01-04T17:39:50",null,"Nature de la finition","Description de la finition y compris la teinte ","Vernis, huilé, brut","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{63A09CB5-32A3-420C-9E06-50D1AE0008B5}","GTTE Façades","2018-01-04T17:39:54",null,"Type de teinte de la finition","Type de teinte de la finition","Gris clair, chene miel, …","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{6F0B2A28-5221-43FD-A1AC-1B8B0D1A0280}","GTTE Façades","2018-01-04T17:39:57",null,"Mise en œuvre de la finition","Mise en œuvre de la finition en atelier ou sur chantier","Atelier, chantier","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{3B36EB41-39A4-4649-837C-BD21D70A4B31}","P08-302","2018-01-09T10:05:39",null,"Satisfaction aux exigences de résistance aux chocs","Capacité du système de bardage conforme au DTU 41.2 à satisfaire aux exigences de chocs de sécurité et de conservation de performances","to be defined","To be defined","boolean-type",1,"sans grandeur","Oui\nNon",null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{20A27D3D-11D3-4D92-9DC2-D1E78DBB9761}","GTTE Façades","2018-02-07T12:41:01",null,"Présence d'un pare-pluie","Présence d'un pare-pluie dans le cas d'un bardage double-peau","to be defined","To be defined","boolean-type",1,"sans grandeur","Oui\nNon",null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{B179467D-B497-45CE-9061-401C20272D1B}","NF DTU 41.2\r\n","2017-12-05T16:48:34",null,"Orientation des lames","Orientation des lames (ex: verticales, horizontales, obliques, mixtes)","Angle of cladding","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{D21893C3-EF43-4A0A-AA00-E359D1D915D2}","NF DTU 41.2\r\n","2017-12-06T11:53:27",null,"Type de mise en œuvre du bardage","Type de mise en œuvre du bardage (A recouvrement, à emboitement, à clairevoie, …)","Kind of laying","Type of laying of the cladding","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{F449F0DE-E61D-4855-A949-FE11A7BA2C45}","GTTE Façades","2018-01-04T17:01:37",null,"Essence de bois","Essence de bois des lames","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{BFE45287-5B02-4754-AD15-E37A106E14DB}","FD P 20-651","2017-12-05T17:59:43",null,"Compatibilité classe d'emploi de la lame","Compatibilité avec la classe d'emploi requise dans le projet pour les lames","To be defined","To be defined","enumerated-type",1,"sans grandeur","2\n3.1\n3.2\n4",null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{20A4CA1A-F75F-43A9-9109-67E049EB9AE7}","NF DTU 41.2\r\n","2018-01-04T17:00:53",null,"Classement d'aspect","Classement minimal d'aspect des lames (classe L selon DTU 41.2 pour les résineux, classe A selon NF EN 14951 pour les feuillus, …)","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{78F0FDB0-8FD0-40BA-B76D-8594C30481D0}","NF DTU 41.2\r\n","2017-12-05T18:26:13",null,"Entraxe ossature de bardage","Distance entre 2 ossatures de bardage dans le même plan","Interaxial cladding frame","Distance between 2 siding frames in the same plan","integer-type",1,"longueur",null,"mm",null,"FR","({(0,650)},mm)",null,null,"2018-10-10",null,"Bardage bois"]
["{16FAAEE2-D7F3-4F62-9503-09314EAA4BE5}","NF DTU 41.2\r\n","2017-12-06T10:49:38",null,"Epaisseur du système de bardage","Epaisseur hors-tout du système de bardage","Thickness of the system","To be defined","integer-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{22E63E23-51B8-4864-96B6-AA5C5E1FDF82}","NF DTU 41.2\r\n","2018-01-04T17:22:22",null,"Type de tête des fixations","Type de tête des fixations (ex: têtes plates, têtes bombées, …)","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{4A78ECA3-4E75-4FD3-879B-7F88B50C3D67}","NF DTU 41.2\r\n","2018-01-04T17:45:57",null,"Largeur exposée","Largeur utile (visible) des lames posées (= Largeur Hors-tout moins le recouvrement)","To be defined","To be defined","integer-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{C51429B6-A80A-4498-8A35-CAE910105CC3}","NF DTU 41.2\r\n","2017-12-06T11:49:22",null,"Type de profil des lames","Type de profil des lames","To be defined","To be defined","character-type",1,"sans grandeur",null,"m",null,"FR","({(0,)},m)",null,null,"2018-10-10",null,"Bardage bois"]
["{6D7F3D5A-9343-466E-967D-3D514426698E}","NF DTU 41.2\r\n","2017-12-06T11:21:17",null,"Nature de la fixation du bardage sur l'ossature","Type de fixation prévue pour assembler le bardage et l'ossature","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{18B7DE33-4C96-4D20-BC03-307AC316F3CF}","NF DTU 26.1","2018-02-07T15:09:46",null,"Résistance à l'arrachement","Résistance à l'arrachement","To be defined","To be defined","enumerated-type",1,"sans grandeur","Rt3 (Rt > 0,8 MPa)\nRt2 (0,6 MPa ≤ Rt ≤ 0,8 MPa)\nRt1 (0,4 MPa ≤ Rt < 0,6 MPa)",null,null,"FR",null,null,null,"2018-10-10",null,"Enduits"]
["{DCB0D308-3D1E-40AD-92FC-8ED911A3B989}","NF DTU 26.1","2018-02-07T15:10:31",null,"Compatibilité de l'enduit au support","Compatibilité de l'enduit au support","To be defined","To be defined","boolean-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Enduits"]
["{61715A85-4D33-4C3E-A4C5-B46F7C61D878}","NF DTU 26.1","2018-02-07T15:11:12",null,"Résistance mécanique de l'enduit","Résistance mécanique de l'enduit conditionnée par le dosage en liants","Resistance to tearing of the support","Ability of the support to receive a coating ( The minimum tear resistance is measured by direct pulling)","real-type",1,"contrainte",null,null,null,"FR",null,null,null,"2018-10-10",null,"Enduits"]
["{3800973C-DA4E-4C3B-BEBA-32C100793345}","NF T 34-722\r\n","2018-02-07T15:21:07",null,"Epaisseur du revêtement","Epaisseur du revêtement","To be defined","To be defined","real-type",1,"longueur",null,"microns",null,"FR",null,null,null,"2018-10-10",null,"Peinture"]
["{DDA619B6-12BF-41AC-A8E8-73E86B0C0C7A}","NF T 34-722\r\n","2018-02-07T15:23:25",null,"Perméabilité à la vapeur d'eau","Perméabilité à la vapeur d'eau","To be defined","To be defined","boolean-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{ABE90E1B-C133-431B-BC95-23E927D2AD19}","GTTE Façades","2018-01-09T10:44:45",null,"Essence de bois des éléments d'ossatures","Essence de bois des éléments d'ossatures","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{0D9490D0-8589-421A-8FFE-00EF7F8A4A62}","GTTE Façades","2018-01-09T10:51:59",null,"Essence de bois des éléments d'ossatures secondaires extérieures","Essence de bois des éléments d'ossatures secondaires extérieures","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{1DF0D867-A091-477A-8EF9-EC97D19F4616}","GTTE Façades","2018-01-09T10:53:12",null,"Essence de bois des éléments ossatures secondaires intérieures","Essence de bois des éléments ossatures secondaires intérieures","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{BE312A55-8B4D-4442-9892-93974CFA6667}","FD P 20-651","2018-01-10T10:53:11.995",null,"Compatibilité classe d'emploi des éléments en bois","Compatibilité avec la classe d'emploi requise pour les éléments d'ossatures primaires et secondaires","To be defined","To be defined","boolean-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{82B28790-06B5-490E-A185-C43A6801F99D}","FD P 20-651","2018-01-09T10:58:47",null,"Compatibilité classe d'emploi de la lisse basse","Compatibilité avec la classe d'emploi requise pour la lisse basse","To be defined","To be defined","boolean-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{0C171828-9377-421E-967A-68079FC445C1}","NF DTU 31.4\r\n","2018-01-09T11:02:25",null,"Resistance aux insectes des éléments en bois","Resistance aux insectes à larves xylophages et/ou termites des éléments en bois","To be defined","To be defined","boolean-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{636D108E-11D3-4795-A9DB-52F155E524B9}","NF DTU 31.4\r\n","2018-01-09T11:25:15",null,"Largeurs des éléments d'ossatures","Largeurs des éléments d'ossatures","To be defined","To be defined","integer-type",1,"longueur",null,"cm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{E460AEAE-F5A3-40B0-813B-B277A1A04754}","NF DTU 31.4\r\n","2018-01-09T11:25:18",null,"Largeurs des éléments d'ossatures secondaires extérieures","Largeurs des éléments d'ossatures secondaires extérieures","To be defined","To be defined","integer-type",1,"longueur",null,"cm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{9DD1EE55-ED88-45F4-A0F9-8189508BEBD3}","NF DTU 31.4\r\n","2018-01-09T11:25:20",null,"Largeurs des éléments d'ossatures secondaires intérieures","Largeurs des éléments d'ossatures secondaires intérieures","To be defined","To be defined","integer-type",1,"longueur",null,"cm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{2A48B8A3-D7B5-40A7-AE92-138D06DC7C84}","NF DTU 31.4\r\n","2017-12-12T15:28:34",null,"Entraxe des éléments d'ossatures","Entraxe des éléments d'ossatures","Interaxial frame","Spacing between frame","integer-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{42F60E09-9598-45BD-9CE5-237608AD5294}","NF DTU 31.4\r\n","2018-01-09T11:24:06",null,"Entraxe des éléments d'ossatures secondaires extérieures","Entraxe des éléments d'ossatures secondaires extérieures","To be defined","To be defined","integer-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{C7CF1097-00EA-4638-A076-1AF97AAD22B1}","NF DTU 31.4\r\n","2018-01-09T11:24:08",null,"Entraxe des éléments d'ossatures secondaires intérieures","Entraxe des éléments d'ossatures secondaires intérieures","To be defined","To be defined","integer-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{59E181D9-55A0-49DA-A55C-756A05953F84}","NF DTU 31.4\r\n","2018-01-09T11:35:22",null,"Orientation des éléments d'ossatures","Orientation des éléments d'ossatures verticaux et horizontaux","To be defined","To be defined","enumerated-type",1,"sans grandeur","verticaux\nhorizontaux",null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{CF62A7B4-8977-48EC-BE94-5A81274F1A1C}","NF DTU 31.4\r\n","2018-01-09T11:35:25",null,"Orientation des éléments d'ossatures secondaires extérieures","Orientation des éléments d'ossatures secondaires extérieures verticaux et horizontaux","To be defined","To be defined","enumerated-type",1,"sans grandeur","verticaux\nhorizontaux",null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{CF8BCCE1-13C5-4A8B-8EAC-50268526F147}","NF DTU 31.4\r\n","2018-01-09T11:35:28",null,"Orientation des éléments d'ossatures secondaires intérieures","Orientation des éléments d'ossatures secondaires intérieures verticaux et horizontaux","To be defined","To be defined","enumerated-type",1,"sans grandeur","verticaux\nhorizontaux",null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{D6EB3364-4965-4531-8E27-BC4E7E78A736}","NF DTU 31.4\r\n","2017-12-12T15:10:18",null,"Nature du voile de stabilité","Nature du panneau remplissant la fonction de voile de stabilité (ex: contreplaqué type 3S, panneau particules P5, panneau de particules P7, OSB 3, OSB 4, LVL 2S, LVL 3S)","Stability shear wall","Type of panel used for stability shear wall","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{D1E6921D-0303-4A18-931A-021C77FA59DC}","GTTE Façades","2018-01-09T11:38:45",null,"Epaisseur du voile de stabilité","Epaisseur du panneau remplissant la fonction de voile de stabilité","To be defined","To be defined","integer-type",1,"longueur",null,"cm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{5C60C8D9-0D95-4DC9-9A4E-7FA308C4782A}","GTTE Façades","2018-01-09T12:16:26",null,"Valeur Sd du voile de stabilité","Valeur Sd du voile de stabilité en mètre","To be defined","To be defined","integer-type",1,"longueur",null,"m",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{74997D3F-2C21-44BC-BFF6-DB6D81687070}","NF DTU 31.4\r\n","2017-12-12T16:13:34",null,"Nature du Pare-pluie","Nature du pare-pluie souple ou rigide","Rain-barrier","Sd value for the rain-barrier","enumerated-type",1,"sans grandeur","souple\nrigide",null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{91A24E05-AFB9-47AD-B36A-3702ACE7F746}","GTTE Façades","2018-01-09T11:48:54",null,"Nature du Pare-pluie rigide","Nature du panneau remplissant la fonction d'écran rigide (ex: panneau de fibres de type SB-H ou SB-E ou MDF RWH)","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{3505E3E1-E09A-439E-B6B7-FF79C060A613}","GTTE Façades","2018-01-09T11:53:56",null,"Epaisseur du Pare-pluie rigide","Epaisseur du panneau remplissant la fonction d'écran rigide","To be defined","To be defined","integer-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{E48B2D26-0319-4A06-B2CA-B1AB165AF9D7}","GTTE Façades","2018-01-09T11:57:24","Sd","Valeur Sd du pare-pluie","Valeur Sd du pare-pluie en mètre","To be defined","To be defined","real-type",1,"longueur",null,"m",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{873DA443-402B-4C03-87BE-C53EDA48C7D5}","GTTE Façades","2018-01-09T12:00:12",null,"Résistance aux UV du pare-pluie","Conformité du pare-pluie à satisfaire aux exigences d'étanchéité à l'eau après 5000h d'exposition aux UV","To be defined","To be defined","boolean-type",1,"sans grandeur","Oui\nNon",null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{E550E3E6-4E66-4DBE-A019-6E6784FB8B8F}","GTTE Façades","2018-01-09T11:59:47",null,"Nature de l'isolant entre éléments d'ossatures","Nature de l'isolant semi-rigide entre éléments d'ossatures (ex: laines minérales, fibres végétales…)","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{20E96CDC-3192-49A9-93DD-2FE35F27B526}","GTTE Façades","2018-01-09T12:04:46",null,"Nature de l'isolant du doublage extérieur","Nature de l'isolant semi-rigide entre éléments d'ossatures secondaires extérieures (ex: laines minérales, fibres végétales…)","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{177BB781-3293-45FB-8270-7F849D9D1FCE}","GTTE Façades","2018-01-09T12:04:50",null,"Nature de l'isolant du doublage intérieur","Nature de l'isolant semi-rigide entre éléments d'ossatures secondaires intérieures (ex: laines minérales, fibres végétales…)","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{14631FD0-0F15-42DD-86A3-8793C88B9827}","GTTE Façades","2018-01-09T12:06:34",null,"Epaisseur de l'isolant entre éléments d'ossatures","Epaisseur de l'isolant semi-rigide entre éléments d'ossatures","To be defined","To be defined","real-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{6D231B77-A082-436A-A7DA-AB5C2C3E1C6B}","GTTE Façades","2018-01-09T12:06:36",null,"Epaisseur de l'isolant du doublage extérieur","Epaisseur de l'isolant semi-rigide entre éléments d'ossatures secondaires extérieures","To be defined","To be defined","real-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{F4357B5F-16E5-45E8-8074-A35CA8405D51}","GTTE Façades","2018-01-09T12:06:39",null,"Epaisseur de l'isolant du doublage intérieur","Epaisseur de l'isolant semi-rigide entre éléments d'ossatures secondaires intérieures","To be defined","To be defined","real-type",1,"longueur",null,"mm",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{4E5DF3DE-067F-41E1-9912-0EA0A7CC325D}","GTTE Façades","2018-01-09T12:06:55",null,"Conductivité thermique de l'isolant entre éléments d'ossatures","Conductivité thermique de l'isolant semi-rigide entre éléments d'ossatures","To be defined","To be defined","real-type",1,"conductivité thermique",null,null,null,"FR",null,null,null,"2018-10-10","propriété proposée pour les bardages double peau / voir cohérence avec propriétés créées par GT Isolation","Bardage bois","Thermique"]
["{611F3267-70EF-410B-8DCC-1E0877C9638B}","GTTE Façades","2018-01-09T12:06:58",null,"Conductivité thermique de l'isolant du doublage extérieur","Conductivité thermique de l'isolant semi-rigide entre éléments d'ossatures secondaires extérieures","To be defined","To be defined","real-type",1,"conductivité thermique",null,null,null,"FR",null,null,null,"2018-10-10","propriété proposée pour les bardages double peau / voir cohérence avec propriétés créées par GT Isolation","Bardage bois","Thermique"]
["{1392B810-1E1F-40D2-B11E-97A0D4AF5D6A}","GTTE Façades","2018-01-09T12:07:01",null,"Conductivité thermique du doublage intérieur","Conductivité thermique de l'isolant semi-rigide entre éléments d'ossatures secondaires intérieures","To be defined","To be defined","real-type",1,"conductivité thermique",null,null,null,"FR",null,null,null,"2018-10-10","propriété proposée pour les bardages double peau / voir cohérence avec propriétés créées par GT Isolation","Bardage bois","Thermique"]
["{E6BE67B6-FF52-422D-983A-AE3259E966F0}","GTTE Façades","2018-01-09T12:10:31",null,"Type de barrière à la diffusion de vapeur d'eau","Composition du sytème faisant office de barrière à la diffusion de la vapeur d'eau (pare-vapeur souple ou panneau à base de bois)","To be defined","To be defined","character-type",1,"sans grandeur",null,null,null,"FR",null,null,null,"2018-10-10",null,"Bardage bois"]
["{8409555A-87F1-4E22-A1A4-CB242BD3DC81}","GTTE Façades","2017-12-12T16:41:24",null,"Résistance thermique de la FOB","Résistance thermique de la façade du pare-pluie au doublage intérieur","Thermal requirements","Thermal resistance of the facade","real-type",1,"coefficient d'isolation thermique",null,"m².K/W",null,"FR",null,null,null,"2018-10-10",null,"Bardage bois","Thermique"]

{"sheet":"Pays d'usage","index":3,"n_rows":255,"n_cols":7,"rows_kept":255,"cut":false,"hidden":false,"merged":[[0,0,0,5],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,4,3,4],[2,5,3,5],[2,6,3,6],[237,0,239,0],[237,1,239,1],[237,2,239,2],[237,3,239,3],[237,4,239,4],[237,5,239,5]]}
[]
[]
["Num.","alpha-3","alpha-2","Codes ISO","Nom français","Nom ISO du pays ou territoire","Nom dans la langue originale, en forme longue (traduction en français)"]
[null,null,null,"régions"]
[4,"AFG","AF","ISO 3166-2:AF"," Afghanistan","AFGHANISTAN","د افغانستان اسلامي دولتدولت اسلامی افغانستان (Da Afghanestan Islami Jomhouriyet) ; جمهوری اسلامی افغانستان (Jomhūrī-ye Eslāmī-ye Afġānestān) ; (République islamique d'Afghanistan)"]
[8,"ALB","AL","ISO 3166-2:AL"," Albanie","ALBANIE","Shqipëri ; Republika e Shqipërisë ; (République d'Albanie)"]
[10,"ATA","AQ","ISO 3166-2:AQ"," Antarctique","ANTARCTIQUE","Traité sur l’Antarctique (entré en vigueur le 1er janvier 1961) ; The Antarctic Treaty ; Tratado Antárctico ; Договор об Антарктике"]
[12,"DZA","DZ","ISO 3166-2:DZ"," Algérie","ALGÉRIE","الجمهورية الجزائرية الديمقراطية الشعبية (République Algérienne Démocratique et Populaire)"]
[16,"ASM","AS","(ISO 3166-2)"," Samoa américaines","SAMOA AMÉRICAINES","Samoa"]
[20,"AND","AD","ISO 3166-2:AD"," Andorre","ANDORRE","Principat d’Andorra (Principauté d’Andorre)"]
[24,"AGO","AO","ISO 3166-2:AO"," Angola","ANGOLA","República de Angola"]
[28,"ATG","AG","ISO 3166-2:AG"," Antigua-et-Barbuda","ANTIGUA-ET-BARBUDA","Antigua and Barbadua"]
[31,"AZE","AZ","ISO 3166-2:AZ"," Azerbaïdjan","AZERBAÏDJAN","Azərbaycan Respublikası"]
[32,"ARG","AR","ISO 3166-2:AR"," Argentine","ARGENTINE","Argentina"]
[36,"AUS","AU","ISO 3166-2:AU"," Australie","AUSTRALIE","Australia"]
[40,"AUT","AT","ISO 3166-2:AT"," Autriche","AUTRICHE","Österreich"]
[44,"BHS","BS","ISO 3166-2:BS"," Bahamas","BAHAMAS","Commonwealth of the Bahamas"]
[48,"BHR","BH","ISO 3166-2:BH"," Bahreïn","BAHREÏN","مملكة البحرين (Mamlakat al-Bahrayn)"]
[50,"BGD","BD","ISO 3166-2:BD"," Bangladesh","BANGLADESH","গণপ্রজাতন্ত্রী বাংলাদেশ (Gônoprojatontri Bangladesh)"]
[51,"ARM","AM","ISO 3166-2:AM"," Arménie","ARMÉNIE","Հայաստան (Hayastan)"]
[52,"BRB","BB","ISO 3166-2:BB"," Barbade","BARBADE","Barbados"]
[56,"BEL","BE","ISO 3166-2:BE"," Belgique","BELGIQUE","(Royaume de) Belgique ; (Koninkrijk) België ; (Königreich) Belgien"]
[60,"BMU","BM","ISO 3166-2:BM"," Bermudes","BERMUDES","Bermuda"]
[64,"BTN","BT","ISO 3166-2:BT"," Bhoutan","BHOUTAN","འབྲུག་ཡུལ (Druk Yul)"]
[68,"BOL","BO","ISO 3166-2:BO"," Bolivie","BOLIVIE, ÉTAT PLURINATIONAL DE","(Estado Plurinacional de / República de) Bolivia ; Bulibiya Mama llaqta ; Wuliwya Suyu ; Tetã Volívia"]
[70,"BIH","BA","ISO 3166-2:BA"," Bosnie-Herzégovine","BOSNIE-HERZÉGOVINE","Republika Bosna i Hercegovina"]
[72,"BWA","BW","ISO 3166-2:BW"," Botswana","BOTSWANA","Republic of Botswana ; Lefatshe la Botswana"]
[74,"BVT","BV","ISO 3166-2:BV"," Île Bouvet","BOUVET, ÎLE","Bouvetøya"]
[76,"BRA","BR","ISO 3166-2:BR"," Brésil","BRÉSIL","República Federativa do Brasil"]
[84,"BLZ","BZ","ISO 3166-2:BZ"," Belize","BELIZE","Belize"]
[86,"IOT","IO","(ISO 3166-2)"," Territoire britannique de l'océan Indien","OCÉAN INDIEN, TERRITOIRE BRITANNIQUE DE L'"]
[90,"SLB","SB","(ISO 3166-2)"," Salomon","SALOMON, ÎLES","Salomons Islands"]
[92,"VGB","VG","(ISO 3166-2)"," Îles Vierges britanniques","ÎLES VIERGES BRITANNIQUES","British Virgin Islands"]
[96,"BRN","BN","ISO 3166-2:BN"," Brunei","BRUNÉI DARUSSALAM","بروني دارالسلام (Negara Brunei Darussalam) ; State of Brunei Darussalam"]
[100,"BGR","BG","ISO 3166-2:BG"," Bulgarie","BULGARIE","Република България (Republika Bălgaria)"]
[104,"MMR","MM","(ISO 3166-2)"," Birmanie","MYANMAR","Union of Myanmar"]
[108,"BDI","BI","ISO 3166-2:BI"," Burundi","BURUNDI","République du Burundi ; Republika y’Uburundi"]
[112,"BLR","BY","ISO 3166-2:BY"," Biélorussie","BÉLARUS","Беларусь (Belarusy)"]
[116,"KHM","KH","ISO 3166-2:KH"," Cambodge","CAMBODGE","ព្រះរាជាណាចក្រកម្ពុជា (Preăh Réachéanachâkr Kâmpŭchea)"]
[120,"CMR","CM","ISO 3166-2:CM"," Cameroun","CAMEROUN","Cameroun ; Cameroon"]
[124,"CAN","CA","ISO 3166-2:CA"," Canada","CANADA","Canada ; Canada"]
[132,"CPV","CV","ISO 3166-2:CV"," Cap-Vert","CABO VERDE","Cabo Verde"]
[136,"CYM","KY","ISO 3166-2:KY"," Îles Caïmans","CAÏMANES, ÎLES","Cayman Islands"]
[140,"CAF","CF","ISO 3166-2:CF"," République centrafricaine","CENTRAFRICAINE, RÉPUBLIQUE","République centrafricaine ; Ködörösêse tî Bêafrîka"]
[144,"LKA","LK","(ISO 3166-2)"," Sri Lanka","SRI LANKA","Prajatantrika Samajavadi Janarajaya ; Ilankai Sananayaka Sosolisa Kudiyarasu"]
[148,"TCD","TD","(ISO 3166-2)"," Tchad","TCHAD","جمهورية تشاد (Jumhūriyyat Tshād) ; République du Tchad"]
[152,"CHL","CL","ISO 3166-2:CL"," Chili","CHILI","Chile"]
[156,"CHN","CN","ISO 3166-2:CN"," Chine","CHINE","中华人民共和国 (Zhōnghuá Rénmín Gònghéguó)"]
[158,"TWN","TW","(ISO 3166-2)"," Taïwan / (République de Chine (Taïwan))","TAÏWAN, PROVINCE DE CHINE","台灣 ; 臺灣 ; 台湾 (Táiwān) ; (anciennement Formose)"]
[162,"CXR","CX","ISO 3166-2:CX"," Île Christmas","CHRISTMAS, ÎLE","Christmas Islands"]
[166,"CCK","CC","ISO 3166-2:CC"," Îles Cocos","COCOS (KEELING), ÎLES","Territory of Cocos Island"]
[170,"COL","CO","ISO 3166-2:CO"," Colombie","COLOMBIE","Colombia"]
[174,"COM","KM","ISO 3166-2:KM"," Comores (pays)","COMORES","Union des Comores ; جزر القُمُر (Juzur al-Qumur) ; Udzima wa Komori"]
[175,"MYT","YT","(ISO 3166-2)"," Mayotte","MAYOTTE","Mayotte"]
[178,"COG","CG","ISO 3166-2:CG"," République du Congo","CONGO","République du Congo ; Repubilika ya Kongo ; Republiki ya Kongó ; (Congo-Brazzaville)"]
[180,"COD","CD","ISO 3166-2:CD"," République démocratique du Congo","CONGO, LA RÉPUBLIQUE DÉMOCRATIQUE DU","République démocratique du Congo ; Repubilika ya Kongo Demokratiki ; Jamhuri ya Kidemokrasia ya Kongo ; Republiki ya Kongó Demokratiki ; Ditunga dia Kongu wa Mungalaata ; (Congo-Kinshasa, ex-Zaïre)"]
[184,"COK","CK","ISO 3166-2:CK"," Îles Cook","COOK, ÎLES","Cook Islands"]
[188,"CRI","CR","ISO 3166-2:CR"," Costa Rica","COSTA RICA","República de Costa Rica"]
[191,"HRV","HR","ISO 3166-2:HR"," Croatie","CROATIE","Republika Hrvatska"]
[192,"CUB","CU","ISO 3166-2:CU"," Cuba","CUBA","República de Cuba"]
[196,"CYP","CY","ISO 3166-2:CY"," Chypre (pays)","CHYPRE","Κύπρος (Kýpros) ; Kıbrıs ; Κυπριακή Δημοκρατία (Kypriakí Dimokratía) ; Kibris Cumhuriyeti"]
[203,"CZE","CZ","(ISO 3166-2)"," Tchéquie","TCHÉQUIE","Česká republika (République tchèque)"]
[204,"BEN","BJ","ISO 3166-2:BJ"," Bénin","BÉNIN","Bénin ; Orílẹ̀-èdè Olómìnira ilẹ̀ Benin"]
[208,"DNK","DK","ISO 3166-2:DK"," Danemark","DANEMARK","Kongeriget Danmark"]
[212,"DMA","DM","ISO 3166-2:DM"," Dominique","DOMINIQUE","Commonwealth of Dominica"]
[214,"DOM","DO","ISO 3166-2:DO"," République dominicaine","DOMINICAINE, RÉPUBLIQUE","República Dominicana"]
[218,"ECU","EC","ISO 3166-2:EC"," Équateur (pays)","ÉQUATEUR","República del Ecuador"]
[222,"SLV","SV","ISO 3166-2:SV"," Salvador","EL SALVADOR","República de El Salvador"]
[226,"GNQ","GQ","(ISO 3166-2)"," Guinée équatoriale","GUINÉE ÉQUATORIALE","República de Guiena ecuatorial ; République de Guinée équatoriale ; República da Guiné Equatorial"]
[231,"ETH","ET","ISO 3166-2:ET"," Éthiopie","ÉTHIOPIE","የኢትዮጵያ ፌዴራላዊ ዲሞክራሲያዊ ሪፐብሊክ (YeItyopya Fédéralawi Dimokrasiyawi Ripeblik)"]
[232,"ERI","ER","ISO 3166-2:ER"," Érythrée","ÉRYTHRÉE","ሃገረ ኤርትራ (Hagere Ertra) ; دولة إرتريا (Dawlat Iritriyá) ; State of Eritrea"]
[233,"EST","EE","ISO 3166-2:EE"," Estonie","ESTONIE","Eesti"]
[234,"FRO","FO","ISO 3166-2:FO"," Îles Féroé","FÉROÉ, ÎLES","Føroyar ; Færøerne"]
[238,"FLK","FK","ISO 3166-2:FK"," Malouines","FALKLAND, ÎLES (MALVINAS)","Falkland Islands"]
[239,"SGS","GS","(ISO 3166-2)"," Géorgie du Sud-et-les Îles Sandwich du Sud","GÉORGIE DU SUD ET LES ÎLES SANDWICH DU SUD","Géorgie du Sud-et-les Îles Sandwich du Sud"]
[242,"FJI","FJ","ISO 3166-2:FJ"," Fidji","FIDJI","Republic of Fiji ; Matanitu ko Viti ; फ़िजी द्वीप समूह गणराज्य (Fiji Dvip Qamooh Ganarajya)"]
[246,"FIN","FI","ISO 3166-2:FI"," Finlande","FINLANDE","Suomen Tasavalta"]
[248,"ALA","AX","ISO 3166-2:AX"," Îles Åland","ÅLAND, ÎLES","Landskapet Åland ; Ahvenanmaan maakunta ; (État libre associé d'Åland)"]
[250,"FRA","FR","ISO 3166-2:FR"," France","FRANCE","République française"]
[254,"GUF","GF","(ISO 3166-2)"," Guyane","GUYANE FRANÇAISE","Guyane"]
[258,"PYF","PF","(ISO 3166-2)"," Polynésie française","POLYNÉSIE FRANÇAISE","Polynésie française ; Pōrīnetia Farāni "]
[260,"ATF","TF","(ISO 3166-2)"," Terres australes et antarctiques françaises","TERRES AUSTRALES FRANÇAISES","Terres australes et antarctiques françaises"]
[262,"DJI","DJ","ISO 3166-2:DJ"," Djibouti","DJIBOUTI","République de Djibouti ; جمهورية جيبوتي (Jumhūriyyat Jībūtī) ; Gabuutih Ummuuno ; Jamahuuriyada Jabuuti"]
[266,"GAB","GA","(ISO 3166-2)"," Gabon","GABON","République gabonaise"]
[268,"GEO","GE","(ISO 3166-2)"," Géorgie (pays)","GÉORGIE","საქართველო ('Sakartvelo')"]
[270,"GMB","GM","(ISO 3166-2)"," Gambie","GAMBIE","Republic of Gambia"]
[275,"PSE","PS","(ISO 3166-2)"," Palestine","ÉTAT DE PALESTINE","دولة فلسطين (Dawlat Filasţīn)"]
[276,"DEU","DE","ISO 3166-2:DE"," Allemagne","ALLEMAGNE","Bundesrepublik Deutschland (République Fédérale d'Allemagne)"]
[288,"GHA","GH","(ISO 3166-2)"," Ghana","GHANA","Republic of Ghana"]
[292,"GIB","GI","(ISO 3166-2)"," Gibraltar","GIBRALTAR"]
[296,"KIR","KI","(ISO 3166-2)"," Kiribati","KIRIBATI","Kiribati"]
[300,"GRC","GR","(ISO 3166-2)"," Grèce","GRÈCE","Ελλάδα (Ellinikí Dimokratía)"]
[304,"GRL","GL","(ISO 3166-2)"," Groenland","GROENLAND","Kalaallit Nunaat ; Grønland"]
[308,"GRD","GD","(ISO 3166-2)"," Grenade (pays)","GRENADE","Commonwealth of Grenada"]
[312,"GLP","GP","(ISO 3166-2)"," Guadeloupe","GUADELOUPE"]
[316,"GUM","GU","(ISO 3166-2)"," Guam","GUAM","Guam ; Guåhån"]
[320,"GTM","GT","(ISO 3166-2)"," Guatemala","GUATEMALA","República de Guatemala"]
[324,"GIN","GN","(ISO 3166-2)"," Guinée","GUINÉE","République de Guinée"]
[328,"GUY","GY","(ISO 3166-2)"," Guyana","GUYANA","Co-Operative Republic of Guyana ; (République coopérative du Guyana)"]
[332,"HTI","HT","(ISO 3166-2)"," Haïti","HAÏTI","Repiblik d'Ayiti ; République d'Haïti"]
[334,"HMD","HM","(ISO 3166-2)"," Îles Heard-et-MacDonald","HEARD ET MACDONALD, ÎLES","Heard Island and McDonald Islands"]
[336,"VAT","VA","(ISO 3166-2)"," Saint-Siège (État de la Cité du Vatican)","SAINT-SIÈGE (ÉTAT DE LA CITÉ DU VATICAN)","Stato della Città del Vaticano"]
[340,"HND","HN","(ISO 3166-2)"," Honduras","HONDURAS","República de Honduras"]
[344,"HKG","HK","(ISO 3166-2)"," Hong Kong","HONG KONG","Hong Kong ; 香港 (Jyutping : Hoeng1 Gong2 ; Yale : Hēunggóng) ; 香港 (Hiông-Kóng) ; Hiong-kang ; 香港 (pinyin : Xiānggǎng) ; 香港特別行政區 ; 香港特别行政区 ; Hong Kong Special Administrative Region of the People's Republic of China ; (Région administrative spéciale de Hong Kong de la République populaire de Chine)"]
[348,"HUN","HU","(ISO 3166-2)"," Hongrie","HONGRIE","Magyar"]
[352,"ISL","IS","(ISO 3166-2)"," Islande","ISLANDE","Ísland"]
[356,"IND","IN","(ISO 3166-2)"," Inde","INDE","Republic of India"]
[360,"IDN","ID","(ISO 3166-2)"," Indonésie","INDONÉSIE","Republik Indonesia"]
[364,"IRN","IR","(ISO 3166-2)"," Iran","IRAN, RÉPUBLIQUE ISLAMIQUE D'","جمهوری اسلامی ايران (Jomhūrī-ye Eslāmī-ye Īrān)"]
[368,"IRQ","IQ","(ISO 3166-2)"," Irak","IRAQ","العراق (Al `Irāq)"]
[372,"IRL","IE","(ISO 3166-2)"," Irlande (pays)","IRLANDE","Éire ; Ireland"]
[376,"ISR","IL","(ISO 3166-2)"," Israël","ISRAËL","מְדִינַת יִשְׂרָאֵל (Medinat Yisra'el) ; دولة إسرائيل (Dawlat Isrā'īl)"]
[380,"ITA","IT","(ISO 3166-2)"," Italie","ITALIE","Italia"]
[384,"CIV","CI","ISO 3166-2:CI"," Côte d'Ivoire","CÔTE D’IVOIRE","Côte d’Ivoire"]
[388,"JAM","JM","(ISO 3166-2)"," Jamaïque","JAMAÏQUE","Jamaïca"]
[392,"JPN","JP","(ISO 3166-2)"," Japon","JAPON","日本国 (Nihon Koku))"]
[398,"KAZ","KZ","(ISO 3166-2)"," Kazakhstan","KAZAKHSTAN","Қазақстан Республикасы (Qazaqstan Respublïkası)"]
[400,"JOR","JO","(ISO 3166-2)"," Jordanie","JORDANIE","المملكة الأردنّيّة الهاشميّة (Al Mamlakah al Urduniyah al Hashimiyah)"]
[404,"KEN","KE","(ISO 3166-2)"," Kenya","KENYA","Jamhuri ya Kenya ; Republic of Kenya"]
[408,"PRK","KP","ISO 3166-2:KP"," Corée du Nord","CORÉE, RÉPUBLIQUE POPULAIRE DÉMOCRATIQUE DE","조선민주주의인민공화국 (Chosŏn Minjujuŭi Inmin Konghwaguk) ; 朝鮮民主主義人民共和國"]
[410,"KOR","KR","ISO 3166-2:KR"," Corée du Sud","CORÉE, RÉPUBLIQUE DE","대한민국 (Daehan Min-guk) ; 大韓民國"]
[414,"KWT","KW","(ISO 3166-2)"," Koweït","KOWEÏT","دولة الكويت (Dawlat al Kuwayt)"]
[417,"KGZ","KG","(ISO 3166-2)"," Kirghizistan","KIRGHIZISTAN","Кыргыз Республикасы (Kırgız Respublikası) ; Кыргызская республика (Kyrgyzskaya Respublika)"]
[418,"LAO","LA","(ISO 3166-2)"," Laos","LAO, RÉPUBLIQUE DÉMOCRATIQUE POPULAIRE","ສາທາລະນະລັດ ປະຊາທິປະໄຕ ປະຊາຊົນລາວ (Sathalanalat Passathipatai Passasson lao)"]
[422,"LBN","LB","(ISO 3166-2)"," Liban","LIBAN","République du Liban ; الجمهوريّةاللبنانيّة"]
[426,"LSO","LS","(ISO 3166-2)"," Lesotho","LESOTHO","Muso oa Lesotho ; Kingdom of Lesotho"]
[428,"LVA","LV","(ISO 3166-2)"," Lettonie","LETTONIE","Latvijas"]
[430,"LBR","LR","(ISO 3166-2)"," Liberia","LIBÉRIA","Republic of Liberia"]
[434,"LBY","LY","(ISO 3166-2)"," Libye","LIBYE","دولة ليبيا (Dawlat Lībiyya) ; ⵍⵉⴱⵢⴰ (Lībya)"]
[438,"LIE","LI","(ISO 3166-2)"," Liechtenstein","LIECHTENSTEIN","Fürstentum Liechtenstein"]
[440,"LTU","LT","(ISO 3166-2)"," Lituanie","LITUANIE","Lietuvos Respublika ; Lietuva"]
[442,"LUX","LU","(ISO 3166-2)"," Luxembourg (pays)","LUXEMBOURG","Groussherzogtum Lëtzebuerg ; Grand Duché de Luxembourg ; Großherzogtum Luxemburg"]
[446,"MAC","MO","(ISO 3166-2)"," Macao","MACAO","Região Administrativa Especial de Macau da República Popular da China"]
[450,"MDG","MG","(ISO 3166-2)"," Madagascar","MADAGASCAR","République de Madagascar ; Repoblikan'i Madagasikara"]
[454,"MWI","MW","(ISO 3166-2)"," Malawi","MALAWI","Republic of Malawi ; Dziko la Malaŵi"]
[458,"MYS","MY","(ISO 3166-2)"," Malaisie","MALAISIE","Malaysia"]
[462,"MDV","MV","(ISO 3166-2)"," Maldives","MALDIVES","ދިވެހިރާއްޖޭގެ ޖުމްހޫރިއްޔާ (Divehi Rājjey ge Jumhuriyyā)"]
[466,"MLI","ML","(ISO 3166-2)"," Mali","MALI","République du Mali"]
[470,"MLT","MT","(ISO 3166-2)"," Malte","MALTE","Repubblika ta' Malta ; Republic of Malta"]
[474,"MTQ","MQ","(ISO 3166-2)"," Martinique","MARTINIQUE"]
[478,"MRT","MR","(ISO 3166-2)"," Mauritanie","MAURITANIE","République islamique de Mauritanie ; الجمهورية الإسلامية الموريتانية"]
[480,"MUS","MU","(ISO 3166-2)"," Maurice (pays)","MAURICE"]
[484,"MEX","MX","(ISO 3166-2)"," Mexique","MEXIQUE","Estados Unidos Mexicanos"]
[492,"MCO","MC","(ISO 3166-2)"," Monaco","MONACO"]
[496,"MNG","MN","(ISO 3166-2)"," Mongolie","MONGOLIE","Монгол Улс Mongol Uls"]
[498,"MDA","MD","(ISO 3166-2)"," Moldavie","MOLDOVA","Republica Moldova"]
[499,"MNE","ME","(ISO 3166-2)"," Monténégro","MONTÉNÉGRO"]
[500,"MSR","MS","(ISO 3166-2)"," Montserrat","MONTSERRAT","Montserrat"]
[504,"MAR","MA","(ISO 3166-2)"," Maroc","MAROC","المملكة المغربية (Al Mamlakatu'l-Maghribiya) ; ⵜⴰⴳⵍⴷⵉⵜ ⵏ ⵍⵎⴰⵖⵔⵉⴱ (Tagldit n'Lmeġrib)"]
[508,"MOZ","MZ","(ISO 3166-2)"," Mozambique","MOZAMBIQUE","República de Moçambique"]
[512,"OMN","OM","(ISO 3166-2)"," Oman","OMAN","Saltanat Uman ; سلطنة عُمان"]
[516,"NAM","NA","(ISO 3166-2)"," Namibie","NAMIBIE","Namibia"]
[520,"NRU","NR","(ISO 3166-2)"," Nauru","NAURU","Ripublik Naoero ; Republic of Nauru"]
[524,"NPL","NP","(ISO 3166-2)"," Népal","NÉPAL"]
[528,"NLD","NL","(ISO 3166-2)"," Pays-Bas","PAYS-BAS","Nederland"]
[531,"CUW","CW","ISO 3166-2:CW"," Curaçao","CURAÇAO","Curaçao, Kòrsou"]
[533,"ABW","AW","ISO 3166-2:AW"," Aruba","ARUBA","Aruba"]
[534,"SXM","SX","(ISO 3166-2)"," Saint-Martin","SAINT-MARTIN (PARTIE NÉERLANDAISE)"]
[535,"BES","BQ","ISO 3166-2:BQ"," Pays-Bas caribéens","BONAIRE, SAINT-EUSTACHE ET SABA","Bonaire, Sint-Eustatius, en Saba"]
[540,"NCL","NC","(ISO 3166-2)"," Nouvelle-Calédonie","NOUVELLE-CALÉDONIE"]
[548,"VUT","VU","(ISO 3166-2)"," Vanuatu","VANUATU","Ripablik blong Vanuatu ; Republic of Vanuatu ; République de Vanuatu"]
[554,"NZL","NZ","(ISO 3166-2)"," Nouvelle-Zélande","NOUVELLE-ZÉLANDE","New Zeland"]
[558,"NIC","NI","(ISO 3166-2)"," Nicaragua","NICARAGUA","Republica de Nicaragua"]
[562,"NER","NE","(ISO 3166-2)"," Niger","NIGER"]
[566,"NGA","NG","(ISO 3166-2)"," Nigeria","NIGÉRIA"]
[570,"NIU","NU","(ISO 3166-2)"," Niue","NIUÉ","Niue ; Niuē"]
[574,"NFK","NF","(ISO 3166-2)"," Île Norfolk","NORFOLK, ÎLE","Norfolk Island"]
[578,"NOR","NO","(ISO 3166-2)"," Norvège","NORVÈGE","Kongeriket Norge ; Noreg"]
[580,"MNP","MP","(ISO 3166-2)"," Îles Mariannes du Nord","MARIANNES DU NORD, ÎLES","Commonwealth of the Northern Mariana Islands"]
[581,"UMI","UM","(ISO 3166-2)"," Îles mineures éloignées des États-Unis","ÎLES MINEURES ÉLOIGNÉES DES ÉTATS-UNIS","United States Minor Outlying Islands"]
[583,"FSM","FM","(ISO 3166-2)"," Micronésie (pays)","MICRONÉSIE, ÉTATS FÉDÉRÉS DE","Micronesia"]
[584,"MHL","MH","(ISO 3166-2)"," Îles Marshall (pays)","MARSHALL, ÎLES","Aolepān Aorōkin M̧ajeļ ; Republic of the Marshall Islands"]
[585,"PLW","PW","(ISO 3166-2)"," Palaos","PALAOS","Republic of Palau ; Beluu er a Belau"]
[586,"PAK","PK","(ISO 3166-2)"," Pakistan","PAKISTAN","Islami Jamhuria Pakistan ; اسلامی جمہوریت پاکستان"]
[591,"PAN","PA","(ISO 3166-2)"," Panama","PANAMA","República de Panamá"]
[598,"PNG","PG","(ISO 3166-2)"," Papouasie-Nouvelle-Guinée","PAPOUASIE-NOUVELLE-GUINÉE","l'État indépendant de Papouasie-Nouvelle-Guinée ; The independent State of Papua New Guinea ; Independen Stet bilong Papua Niugini"]
[600,"PRY","PY","(ISO 3166-2)"," Paraguay","PARAGUAY","República del Paraguay ; Tetä Paraguáype"]
[604,"PER","PE","(ISO 3166-2)"," Pérou","PÉROU","Peru"]
[608,"PHL","PH","(ISO 3166-2)"," Philippines","PHILIPPINES","Republika ng Pilipinas"]
[612,"PCN","PN","(ISO 3166-2)"," Îles Pitcairn","PITCAIRN"]
[616,"POL","PL","(ISO 3166-2)"," Pologne","POLOGNE","Polska"]
[620,"PRT","PT","(ISO 3166-2)"," Portugal","PORTUGAL","Portugal"]
[624,"GNB","GW","(ISO 3166-2)"," Guinée-Bissau","GUINÉE-BISSAU","República da Guiné-Bissau"]
[626,"TLS","TL","(ISO 3166-2)"," Timor oriental","TIMOR-LESTE","Repúblika Demokrátika Timor Lorosa'e ; República Democrática de Timor-Leste"]
[630,"PRI","PR","(ISO 3166-2)"," Porto Rico","PORTO RICO","Estado Libre Asociado de Puerto Rico ; Commonwealth of Puerto Rico"]
[634,"QAT","QA","(ISO 3166-2)"," Qatar","QATAR","دولة قطر (Dawlat Qatar)"]
[638,"REU","RE","(ISO 3166-2)"," La Réunion","RÉUNION","La Réunion"]
[642,"ROU","RO","(ISO 3166-2)"," Roumanie","ROUMANIE","România"]
[643,"RUS","RU","(ISO 3166-2)"," Russie","RUSSIE, FÉDÉRATION DE","Российская Федерация -Rossiiskaïa Fédératsiya"]
[646,"RWA","RW","(ISO 3166-2)"," Rwanda","RWANDA","Repubulika y'u Rwanda ; République Rwandaise"]
[652,"BLM","BL","(ISO 3166-2)"," Saint-Barthélemy","SAINT-BARTHÉLEMY"]
[654,"SHN","SH","(ISO 3166-2)"," Sainte-Hélène, Ascension et Tristan da Cunha","SAINTE-HÉLÈNE, ASCENSION ET TRISTAN DA CUNHA","Saint Helena"]
[659,"KNA","KN","(ISO 3166-2)"," Saint-Christophe-et-Niévès","SAINT-KITTS-ET-NEVIS"]
[660,"AIA","AI","ISO 3166-2:AI"," Anguilla","ANGUILLA","Anguilla"]
[662,"LCA","LC","(ISO 3166-2)"," Sainte-Lucie","SAINTE-LUCIE","Commonwealth of Saint Lucia"]
[663,"MAF","MF","(ISO 3166-2)"," Saint-Martin","SAINT-MARTIN (PARTIE FRANÇAISE)"]
[666,"SPM","PM","(ISO 3166-2)"," Saint-Pierre-et-Miquelon","SAINT-PIERRE-ET-MIQUELON"]
[670,"VCT","VC","(ISO 3166-2)"," Saint-Vincent-et-les Grenadines","SAINT-VINCENT-ET-LES-GRENADINES","Saint Vincent and the Grenadines"]
[674,"SMR","SM","(ISO 3166-2)"," Saint-Marin","SAINT-MARIN","San Marino"]
[678,"STP","ST","(ISO 3166-2)"," Sao Tomé-et-Principe","SAO TOMÉ-ET-PRINCIPE","República Democrática de São Tomé e Príncipe"]
[682,"SAU","SA","ISO 3166-2:SA"," Arabie saoudite","ARABIE SAOUDITE","المملكة العربية السعودية (Mamlakah al `Arabiyahas Su`udiyah)"]
[686,"SEN","SN","(ISO 3166-2)"," Sénégal","SÉNÉGAL","République du Sénégal"]
[688,"SRB","RS","(ISO 3166-2)"," Serbie","SERBIE","Република Србија ; Republika Srbija"]
[690,"SYC","SC","(ISO 3166-2)"," Seychelles","SEYCHELLES","Repiblik Sesel ; Republic of Seychelles ; République des Seychelles"]
[694,"SLE","SL","(ISO 3166-2)"," Sierra Leone","SIERRA LEONE","Sierra Leone"]
[702,"SGP","SG","(ISO 3166-2)"," Singapour","SINGAPOUR","Republic of Singapore (anglais), Republik Singapura (malais), Cingkappūrā Kudiyaracu (tamoul), Xīnjīapō Gònghégúo (chinois)"]
[703,"SVK","SK","(ISO 3166-2)"," Slovaquie","SLOVAQUIE","Slovenská republika (République slovaque)"]
[704,"VNM","VN","(ISO 3166-2)"," Viêt Nam","VIET NAM","Cộng Hoà Xã Hội Chủ Nghĩa Việt Nam ; la République socialiste du Viet Nam"]
[705,"SVN","SI","(ISO 3166-2)"," Slovénie","SLOVÉNIE","Republika Slovenija (République de Slovénie)"]
[706,"SOM","SO","(ISO 3166-2)"," Somalie","SOMALIE","la République fédérale de Somalie ; Jamhuuriyadda Federaalka Soomaaliya ; جمهورية الصومال الفدرالية ; the Federal Republic of Somalia"]
[710,"ZAF","ZA","ISO 3166-2:ZA"," Afrique du Sud","AFRIQUE DU SUD","Republic of South Africa ; Republiek van Suid-Afrika ; IRiphabliki yaseMzantsi Afrika ; IRiphabliki yaseNingizimu Afrika ; IRiphabliki yeSewula Afrika ; (République d'Afrique du Sud)"]
[716,"ZWE","ZW","(ISO 3166-2)"," Zimbabwe","ZIMBABWE","Republic of Zimbabwe"]
[724,"ESP","ES","ISO 3166-2:ES"," Espagne","ESPAGNE","España"]
[728,"SSD","SS","(ISO 3166-2)"," Soudan du Sud","SOUDAN DU SUD","Republic of South Sudan"]
[729,"SDN","SD","(ISO 3166-2)"," Soudan","SOUDAN","Jumhuriyat al-Sudan ; جمهورية السودان"]
[732,"ESH","EH","(ISO 3166-2)"," République arabe sahraouie démocratique","SAHARA OCCIDENTAL"]
[740,"SUR","SR","(ISO 3166-2)"," Suriname","SURINAME","Republiek Suriname"]
[744,"SJM","SJ","(ISO 3166-2)"," Svalbard et ile Jan Mayen","SVALBARD ET ÎLE JAN MAYEN","Svalbard og Jan Mayen"]
[748,"SWZ","SZ","(ISO 3166-2)"," Swaziland","SWAZILAND","Umbuso we Swatini ; Kingdom of Swaziland"]
[752,"SWE","SE","(ISO 3166-2)"," Suède","SUÈDE","Sverige"]
[756,"CHE","CH","(ISO 3166-2)"," Suisse","SUISSE","Confœderatio Helvetica ; Schweizerische Eidgenossenschaft ; Confédération suisse ; Confederazione Svizzera ; Confederaziun svizra ;"]
[760,"SYR","SY","(ISO 3166-2)"," Syrie","SYRIENNE, RÉPUBLIQUE ARABE","الجمهوريّة العربيّة السّوريّة (Al-Jumhūriyyah al-‘Arabīyyah as-Sūriyyah)"]
[762,"TJK","TJ","(ISO 3166-2)"," Tadjikistan","TADJIKISTAN","Ҷумҳурии Тоҷикистон (Jumhurii Tojikiston) ; Респу́блика Таджикиста́н (Respúblika Tadshikistán)"]
[764,"THA","TH","(ISO 3166-2)"," Thaïlande","THAÏLANDE","ราชอาณาจักรไทย (Ratcha Anachak Thai)"]
[768,"TGO","TG","(ISO 3166-2)"," Togo","TOGO","République togolaise"]
[772,"TKL","TK","(ISO 3166-2)"," Tokelau","TOKELAU","Tokelau"]
[776,"TON","TO","(ISO 3166-2)"," Tonga","TONGA","Pule'anga Fakatu'i 'o Tonga ; Kingdom of Tonga"]
[780,"TTO","TT","(ISO 3166-2)"," Trinité-et-Tobago","TRINITÉ-ET-TOBAGO","Republic of Trinidad and Tobago"]
[784,"ARE","AE","ISO 3166-2:AE"," Émirats arabes unis","ÉMIRATS ARABES UNIS","دولة الإمارات العربيّة المتّحدة (al-ʾImārāt al-ʿArabiyyat al-Muttaḥida)"]
[788,"TUN","TN","(ISO 3166-2)"," Tunisie","TUNISIE","الجمهورية التونسية (al-Jumhūriyya at-Tūnisiyya)"]
[792,"TUR","TR","(ISO 3166-2)"," Turquie","TURQUIE","Türkiye Cumhuriyeti"]
[795,"TKM","TM","(ISO 3166-2)"," Turkménistan","TURKMÉNISTAN","Türkmenistan Respublikasy ; Республика Туркменистан (Respublika Turkmenistan)"]
[796,"TCA","TC","(ISO 3166-2)"," Îles Turks-et-Caïcos","TURKS ET CAÏQUES, ÎLES","Turks-and-Caicos"]
[798,"TUV","TV","(ISO 3166-2)"," Tuvalu","TUVALU","Tuvalu ; State of Tuvalu"]
[800,"UGA","UG","(ISO 3166-2)"," Ouganda","OUGANDA","Republic of Uganda ; Jamhuri ya Uganda"]
[804,"UKR","UA","(ISO 3166-2)"," Ukraine","UKRAINE","Украïна (Ukraïna)"]
[807,"MKD","MK","(ISO 3166-2)"," République de Macédoine (pays)","MACÉDOINE, L'EX-RÉPUBLIQUE YOUGOSLAVE DE","Република Македонија"]
[818,"EGY","EG","ISO 3166-2:EG"," Égypte","ÉGYPTE","جمهوريّة مصر العربيّة,"]
[null,null,null,null,null,null,"Gumhuriyyat Miṣr al-ʿArabiyyah,"]
[null,null,null,null,null,null,"(République arabe d’Égypte)"]
[826,"GBR","GB","(ISO 3166-2)"," Royaume-Uni","ROYAUME-UNI","United Kingdom"]
[831,"GGY","GG","(ISO 3166-2)"," Guernesey","GUERNESEY","Guernsey"]
[832,"JEY","JE","(ISO 3166-2)"," Jersey","JERSEY","Bailiwick of Jersey, Bailliage de Jersey"]
[833,"IMN","IM","(ISO 3166-2)"," Île de Man","ÎLE DE MAN","Isle of Man"]
[834,"TZA","TZ","(ISO 3166-2)"," Tanzanie","TANZANIE, RÉPUBLIQUE UNIE DE","United Republic of Tanzania ; Jamhuri ya Muungano wa Tanzania"]
[840,"USA","US","ISO 3166-2:US"," États-Unis","ÉTATS-UNIS","United States of America (USA) ; (États-Unis d'Amérique)"]
[850,"VIR","VI","(ISO 3166-2)"," Îles Vierges des États-Unis","ÎLES VIERGES DES ÉTATS-UNIS","US Virgin Islands"]
[854,"BFA","BF","ISO 3166-2:BF"," Burkina Faso","BURKINA FASO","Burkina Faso"]
[858,"URY","UY","(ISO 3166-2)"," Uruguay","URUGUAY","República Oriental del Uruguay"]
[860,"UZB","UZ","(ISO 3166-2)"," Ouzbékistan","OUZBÉKISTAN","O'zbekiston Respublikasi"]
[862,"VEN","VE","(ISO 3166-2)"," Venezuela","VENEZUELA, RÉPUBLIQUE BOLIVARIENNE DU","República Bolivariana de Venezuela"]
[876,"WLF","WF","(ISO 3166-2)"," Wallis-et-Futuna","WALLIS-ET-FUTUNA","Wallis-et-Futuna"]
[882,"WSM","WS","(ISO 3166-2)"," Samoa","SAMOA","Malo Sa'oloto Tuto'atasi o Samoa ; Independent State of Samoa"]
[887,"YEM","YE","(ISO 3166-2)"," Yémen","YÉMEN","ﺍﻟﺠﻤﻬﻮﺭﯾّﺔ اليمنية"]
[894,"ZMB","ZM","(ISO 3166-2)"," Zambie","ZAMBIE","Republic of Zambia"]

{"sheet":"Grandeurs","index":4,"n_rows":8,"n_cols":2,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Grandeur de base","Symbole de la dimension"]
["longueur","L"]
["masse","M"]
["temps","T"]
["courant électrique","I"]
["température thermodynamique","Θ"]
["quantité de matière","N"]
["intensité lumineuse","J"]

{"sheet":"Modèle d'objet","index":5,"n_rows":5,"n_cols":10,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
["Identifiant unique","Documents de référence","Date de création","Nom dans la langue du créateur","Définition dans la langue du créateur","Nom en anglais international","Définition en anglais international","Représentation visuelle","Pays d'usage","Date de validation"]
[]
[]
["Propriétés associées"]
["Id","Nom dans la langue du créateur"]